

Low Level Utility BrewCMD(W)

The BrewCMD utility is a program to facilitate sending commands to and displaying 
responses from the Brewer. Hence it can be used for simple operation tasks. There are 
two versions of BrewCMD available:

1.	BrewCMD.exe
This version is a DOS based program and works fine with platforms such as W95 
and W98, which are the most common platforms to operate the Brewer.bat 
software. This version of BrewCMD however does not work with WindowsXP.
2.	BrewCMDW.exe
The "W" extension indicates that this program is a Windows based program. This 
version works on XP systems. BrewCMDW does not work on MS-DOS, W95 or 
W89 systems. 

To run the BrewCMD(W) utility the Brewer must be connected via the serial port of the 
PC. The BrewCMD utility is intended for the use of the scientist using the Brewer and 
the technicians installing the Brewer. The BrewCMD utility has three intended functions:

1.  To provide a tool for verifying the validity of connections to the Brewer and 
    for verifying the low level message/response operation of the Brewer.
2.  Uploading firmware and configuration files.
3.  To facilitate sending commands to and displaying responses from the 
    Brewer.
	

Note:	The BrewCMD program is a low level utility. Using this utility can modify the 
calibration and equipment configuration information.


For information on how to upload firmware and configuration file please refer to the 
Service Manual.


